
# AHD-XM350-0239-32X32-V2\_02Interface Description


**CN1** 1 2

**CN2** 1 2 3



**J1** 3 2 1

**J3**  4 3 2 1



**J2**

**4**

**3**

**2**

**1**

、

**Detailed Definition**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Socket | | Specific No. | | Interface Description | Function | |
| CN2 | | 1 | | CVBS | Video Out | |
| 2 | | GND | Ground | |
| 3 | | 12V | 12V DC input | |
| CN1 | | 1 | | IRCUTA | IRCUT | |
| 2 | | IRCUTB |
| J1 | | 1 | | ADC1VIN | Red\_CTRL | |
| 2 | | GND | Ground | |
| 3 | | NC | Undefined | |
| J2 | | 1 | | ALARM\_IN1 | ALARM input | |
| 2 | | GND | Ground | |
| 3 | | 3.3V | 3.3V DC input | |
| 4 | | GND | Ground | |
| J3 | 1 | | GND | | | Ground |
| 2 | | CVI | | | Switch to CVI by grounding |
| 3 | | MODE\_N-P | | | N-P |
| 4 | | TVI | | | Switch to TVI by grounding |