

P2

IRcut

P3 Infrared

P6

Alarm Audio

**not welded**

P7 power&NET

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| sign | Socket | Specific No | Interface Description | Function |
| P2 | J4 | 1 | IC-CUT | IRCUT output |
| 2 | IC-CUT | IRCUT output |
| P3 | J2 | 1 | IRIN\_GPIO1\_7 | IRIN |
| 2 | GND | GND |
| 3 | GPIO2\_0 | GPIO/PWM |
| P6 | J9 | 1 | AC\_OUTL | AC\_OUT |
| 2 | AC\_LINEL | MIC\_P |
| 3 | GND | GND |
| 4 | ALARM\_IN1 | ALARM\_IN |
| 5 | GND | GND |
| P1 | J3 | 1 | LED/PHY\_AD0 | LED |
| 2 | LED/PHY\_AD1 | LED |
| 3 | ETHTX+ | Ethernet signal |
| 4 | ETHTX- | Ethernet signal |
| 5 | ETHRX+ | Ethernet signal |
| 6 | ETHRX- | Ethernet signal |
| 7 | GND | GND |
| 8 | 12V | 12V DC input |